APL LED PL LAMP GUIDE

please ensure the control gear is **bypassed** and the product is fed the 240v supply only , failure to bypass the control gear will cause instant failure of the LED components and render the warranty invalid

PLC TYPE 2 PIN PLL TYPE 4 PIN PLL TYPE 4 PIN

 PLC TYPE 4 PIN

